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EL1242FG-SFP                                     24-Port 10/100+2G SFP Industrial Switch
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YOUR ONE-STOP ICT CONNECTIVITY SOLUTION PROVIDER

[image: ]EL1242FG-SFP is a converging integrated industrial Ethernet unmanaged switch independently developed by our company. This product is mainly developed for the application of point-to-point networks, star networks, tree networks and chain networks in the industrial field. It supports 24-Port 10/100Base-TX and 2 Port 1.25G SFP. This product has a high-performance switching engine, a wavy aluminum alloy shell with an IP40 protection level, a fanless design and an efficient heat dissipation surface, and over-current, over-voltage and EMC protection for the loading power input port. The RJ45 port is equipped with excellent EMC protection performance, so that the series of products can adapt to harsh and dangerous industrial environments. Therefore, it can provide reliable and convenient solutions for users’ Ethernet equipment networking.Interface
· 24*10/100BaseT(X),Automatic detection, Full/half duplex MDI/MDI-x adaptive
· 2 Port 1000Mbps SFP uplink

Industrial conformance
· 12V to 52V DC, redundant power input
· -40℃ to 75℃ operating temperature
· IP40 aluminum housing 
· Supports 6KV DC Ethernet ESD protection
· Supports 6KV DC EFT protection for power line
· Free Fall, Shock and Vibration Stability
· DIN-rail hardware design

SPECIFICATIONS:
	Model No.
	EL1242FG-SFP

	Product description
	24-Port 10/100+2G SFP Industrial Ethernet Switch

	Ethernet interface

	RJ45 Ports
	10/100BaseT(X),Automatic detection,Full/half duplex MDI/MDI-x adaptive

	Standards

	Network Protocols
	IEEE802.3 10BASE-T; 100BASE-T IEEE802.3i 10Base-T;IEEE802.3u;IEEE802.3x;

	Twisted Pair
	10BASE-T: Cat3,4,5 UTP(≤100 meter)
100BASE-TX: Cat5 or later UTP(≤100 meter)

	Switch Properties

	Processing Type:
	Store and Forward

	MAC Table Size
	16K 

	Packet Buffer Size
	4Mbit

	Bandwidth
	14.8G

	Switching Delay
	＜10μs

	Power Consume
	＜10Watts

	Power Parameters

	Power
	Connection: 1 removable 5-contact terminal block(s)
Input voltage: DC12 to 52V redundant dual inputs support reverse connection protection

	LED Indicator
	Power: Green 
Link: Green 

	Physical Characteristics

	Enclosure
	Wavy aluminum alloy

	Protection level
	IP40 

	Dimensions
	150x 126x 53mm （length x width x height)

	Weigh
	0.9kg

	Installation
	Push-in DIN rail

	Environmental Limits

	Operating Temperature
	-40～75℃ （-40～185 °F）

	Storage Temperature 
	-40 to 85°C (-40 to 185°F)

	Ambient Relative Humidity
	5 to 95% (non-condensing)

	Standards and Certifications

	Safety
	EN 62368-1(LVD)

	EMI
	FCC Part 15 Subpart B Class A，EN 55032 Class A

	EMS
	IEC(EN)61000-4-2(ESD): ±8kV Contact, ±8kV Indirect,±15kV Air
IEC(EN)61000-4-3(RS):10V/m(80～1000MHz)
IEC(EN)61000-4-4(EFT): power line:±4kV; data line:±2kV
IEC(EN)61000-4-5(Surge): power:±6kV CM/±4kV DM; data:±4kV
IEC(EN)61000-4-6(RF conduction):3V(10kHz～150kHz),10V(150kHz～80MHz)
IEC(EN)61000-4-16(Common mode conduction):30V cont. 300V,1s
IEC(EN )61000-4-8

	Shock
	IEC 60068-2-27

	Freefall
	IEC 60068-2-32

	Vibration
	IEC 60068-2-6

	MTBF

	Time
	300 000hrs

	Warranty

	Warranty Period
	5 years
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