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EL244GTS                                 24-Port Gigabit +4*10G SFP L3 Managed Industrial Switch
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YOUR ONE-STOP ICT CONNECTIVITY SOLUTION PROVIDER

EL244GTS is a photoelectric convergence integrated Industrial Ethernet Gigabit Managed switch .This product is mainly developed for the application of point-to-point network, star network, tree network, chain network and ring network in the industrial field. With 24 x 10/100/1000Base-TX ports, 4x10G SFP optical ports, all ports support full wire-speed forwarding, and its high-performance switching engine, and has a redundant self-healing ring (fault recovery time＜20ms) to realize single loop, tangent, and intersection loop protocols, support for broadcast storm suppression, port mirroring, port priority QoS settings, port aggregation functions. IP40 rated enclosure, fanless design with highly efficient wavy aluminum alloy shell heat dissipation surface, overcurrent, overvoltage and EMC protection for power inputs, excellent EMC protection for RJ45 ports, to make products work efficiently in harsh industrial environments. And it can provide a reliable and convenient solution for the users’ Ethernet equipment networking.
Product features:
● Data control: Supports 802.3x full-duplex flow control and
network storm suppression 
● Redundant network: supports STP, RSTP, MSTP and ERPS (self-healing time <20ms) 
● Redundancy backup: supports the virtual route redundancy protocol VRRP 
● Multicast management: Support IGMP Snooping V1, V2, and V3 
● VLAN: supports IEEE 802.1Q vlans to effectively isolate broadcast domains 
Link aggregation: Support static/dynamic link aggregation, provide perfect bandwidth utilization 
● QOS: Support COS\DSCP, 4 queues, support WRR\SP scheduling mode 
● Security management: Security management: supports ACL and 802.1x 
● Management: Supports WEB, CLI, and SNMP management 
Monitoring and maintenance: Support port mirroring, interface status monitoring, log management

SPECIFICATIONS:
	Product Name
	24-Port RJ45 +4*10G SFP L3 Managed Industrial Switch

	Model No.
	EL244GTS

	Interface

	RJ45 Port
	24*10/100/1000BaseT(X),Automatic detection, Full/half duplex MDI/MDI-x adaptive

	Optical port
	4*1000/10000Base-FX SFP     

	Console
	RS232

	USB
	USB2.0

	DI/DO
	Relay output, purely resistive load: 5A@30VDC; 8A@250VAC

	Reset
	Short press to reset, long press to restore factory settings

	Power Parameters
	

	Power
	Redundant power Input (DC polarity reverse connection protection and overcurrent protection)
Support any two of following power input:
A:100-240VAC,50/60Hz;110-220VDC (85-264VAC/77-300VDC) ,
B:48VDC (36-75VDC) 
C::12V/24V/36V/48VDC(9.6~60VDC)
Power consumption: max.45W

	LED Indicator
	Power indicator LED : Green PWR
Alarm output LED: Yellow Alarm
System indicator LED: Green SYS
RJ45(Green) Link/Act
SFP(Green) Ulink/Act

	Standards

	Network Protocols
	IEEE802.3-10BaseT,IEEE802.3u-100BaseTX/100Base-FX,IEEE802.3x-Flow Control,IEEE802.3z-1000BaseLX,IEEE802.3ab-1000BaseTX,IEEE802.1ab Logical Link Discovery Protocol,IEEE802.1D-Spanning Tree Protocol,IEEE802.1w-Rapid Spanning Tree Protocol, APS ,IEEE802.1Q -VLAN Tagging, IEEE802.1p -Class of Service,IEEE802.1X-Port Based Network Access Control

	Twisted Pair
	10BASE-T: Cat3,4,5 UTP(≤100 meter)
100BASE-TX: Cat5 or later UTP(≤100 meter)
1000BASE-TX: Cat6 or later UTP(≤100 meter)

	Switch Properties

	Processing Type:
	Store and Forward

	Capacity
	128Gbps

	Packet forwarding rate
	95.232Mpps

	MAC Table Size
	16K 

	Packet Buffer Size
	12Mbit

	Jumbo Frame
	12KB

	Vlan
	4K

	Physical Characteristics

	Protection level
	IP40 

	Enclosure
	Wavy aluminum alloy

	Installation
	Rack mount

	Weigh
	6kg

	Dimensions
	440x304x44mm (L*W*H)

	Environmental Limits

	Working temperature
	-40～75°C（-40～167°F）

	Storage Temperature (package included)
	-40 to 85°C (-40 to 185°F)

	Ambient Relative Humidity
	5 to 95% (non-condensing)

	Standards and Certifications

	Safety
	EN 62368-1(LVD)

	EMI
	FCC Part 15 Subpart B Class A EN 55032 Class A

	EMS
	IEC(EN)61000-4-2(ESD): ±8kV Contact, ±8kV Indirect,±15kV Air
IEC(EN)61000-4-3(RS):10V/m(80～1000MHz)
IEC(EN)61000-4-4(EFT): power line:±4kV; data line:±2kV
IEC(EN)61000-4-5(Surge): power:±6kV CM/±4kV DM; data:±4kV
IEC(EN)61000-4-6(RF conduction):3V(10kHz～150kHz),10V(150kHz～80MHz)
IEC(EN)61000-4-16(Common mode conduction):30V cont. 300V,1s
IEC(EN )61000-4-8

	Shock
	IEC 60068-2-27

	Freefall
	IEC 60068-2-32

	Vibration
	IEC 60068-2-6

	MTBF

	Time
	300 000hrs

	Warranty

	Warranty Period
	5years


SOFTWARE:
	Port Features 
	IEEE 802.3x Flow control

	
	Interface counters

	
	Storm Control

	Link Aggregation 
	Static Aggregation

	
	Dynamic Aggregation, LACP

	
	Supports up to 4 aggregation groups, each group up to 8 ports
Load balancing

	MAC Address Table
	Static MAC Address
MAC Binding

	Mirroring 
	Port-based
One-to-one Mirroring, Many-to-one Mirroring

	Spanning Tree 
	IEEE802.1d STP

	
	IEEE802.1w RSTP

	
	IEEE802.1s MSTP

	ERPS (G.8032) 
	Single Ring, Sub-Ring, Multi-Ring

	
	Recovery Time < 50ms

	LLDP 
	LLDP

	
	LLDP-MED

	Loop Protection 
	Supported

	VLAN 
	4094 VLAN

	
	Port-based VLAN

	
	GVRP

	IGMP 
	Snooping IGMP V1 Snooping

	
	IGMP V2 Snooping

	
	IGMP V3 Snooping

	
	Source Port Check

	
	IGMP Fast Leave

	Security
	

	ACL 
	ACL (IP Standard ACL), IPv4/IPv6

	
	MAC extend ACL

	
	IP extend ACL

	
	L2, L3, L4 fields match

	QoS 
	QoS Class, Remarking

	
	SP, WRR queue scheduling

	
	Ingress port-based rate-limit

	
	Ingress priority-based rate-limit

	
	Egress port-based rate-limit

	
	Egress queue-based rate-limit

	
	Policy-based QoS

	
	Storm Control

	
	8 queues per port

	802.1X
	Port-based

	User management 
	Password protection

	SNMP 
	SNMP V1/V2c/V3

	RMON 
	Statistics Group

	
	History Group

	
	Alarm Group

	
	Events Group

	Web management 
	HTTP V1.1, HTTPS

	Firmware Upgrade 
	Reversion Upgrade

	CLI 
	Support

	Syslog/Debug 
	Support

	Diagnosis 
	Ping (IPv4), ping (IPv6)

	
	Trace route(IPv4)

	Management
	

	NTP 
	SNTP 

	Telnet 
	Telnet Server

	TFTP 
	TFTP Client

	SSH 
	SSH Server
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Order Information
	Specification
	Model No.

	L3 Managed Industrial Switch
24 Port 10/100/1000Base TX+4 Port 10G/1G SFP
	EL244GTS
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