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EL82MGI V3                               8-Port RJ45 +2G SFP L2 Managed Industrial Switch
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YOUR ONE-STOP ICT CONNECTIVITY SOLUTION PROVIDER

EL82MGI V3 is an optical convergence integrated Managed Industrial Ethernet Switch independently developed by our company. This product is mainly developed for the application of point-to-point networks, star networks, tree networks, and chain networks in the industrial field. It supports 8-Port 10/100/1000Base-TX and 2-Port 100/1000Base-FX SFP, and the longest optical communication distance can reach 120KM. 
In addition to its compact size, it has a high-performance switching engine, a wavy aluminum alloy shell with IP40 protection level, a fanless design and efficient heat dissipation surface, and an installed power input terminal over-current, over-voltage, the EL82MGI V3 features DC12-52V redundant power inputs, DIN-rail mounting, high-level EMI/EMC capability, and an operating temperature range of -40 to 75°C available. The EL82MGI V3 has also passed a 100% burn-in test to ensure it will function reliably in the field. Therefore, it can provide reliable and convenient solutions for users’ Ethernet equipment networking.
Interface
· 8*10/100/1000BaseT(X), Automatic detection, Full/half duplex MDI/MDI-x adaptive
· 2*100/1000Base-FX Port SFP
Industrial conformance
· 12V to 52V DC, redundant power input
· -40℃ to 75℃ operating temperature
· IP40 aluminum housing 
· Supports 6KV DC Ethernet ESD protection
· Supports 6KV DC EFT protection for power line
· Free Fall, Shock and Vibration Stability
· DIN-rail hardware design

SPECIFICATIONS:
	Product Name
	8-Port RJ45 +2G SFP L2 Managed Industrial Switch

	Model No.
	EL82MGI V3

	Ethernet interface

	RJ45 Port
	8*10/100/1000BaseT(X),Automatic detection, Full/half duplex MDI/MDI-x adaptive

	Optical port
	2*100/1000Base-FX SFP     

	Power Parameters
	

	Power
	Connection: 1 removable 5-contact terminal block(s)
Input voltage: DC12 to 52V redundant power support reverse connection protection

	Relay out put
	1 set of alarm output relay output

	LED Indicator
	Power indicator light: red P1, P2
Interface indicator light: 
Left of the RJ45: Yellow, Right: Green (Data)
Optical port green Uplink/act indicator light

	Standards

	Network Protocols
	IEEE802.3-10BaseT,IEEE802.3u-100BaseTX/100Base-FX,IEEE802.3x-Flow Control,IEEE802.3z-1000BaseLX,IEEE802.3ab-1000BaseTX,IEEE802.1ab Logical Link Discovery Protocol,IEEE802.1D-Spanning Tree Protocol,IEEE802.1w-Rapid Spanning Tree Protocol, APS ,IEEE802.1Q -VLAN Tagging, IEEE802.1p -Class of Service,IEEE802.1X-Port Based Network Access Control

	Twisted Pair
	10BASE-T: Cat3,4,5 UTP(≤100 meter)
100BASE-TX: Cat5 or later UTP(≤100 meter)
1000BASE-TX: Cat6 or later UTP(≤100 meter)

	Switch Properties

	Processing Type:
	Store and Forward

	Packet forwarding rate
	17.856Mpps

	MAC Table Size
	8K 

	Packet Buffer Size
	4.1Mbit

	Bandwidth
	26G

	Switching Delay
	＜10μs

	Power Consume
	＜15W 

	Physical Characteristics

	Protection level
	IP40 

	Enclosure
	Wavy aluminum alloy

	Installation
	Push-in DIN rail

	Weigh
	0.75kg

	Dimensions
	140x116x42mm (L*W*H)

	Environmental Limits

	Working temperature
	-40～75°C（-40～167°F）

	Storage Temperature (package included)
	-40 to 85°C (-40 to 185°F)

	Ambient Relative Humidity
	5 to 95% (non-condensing)

	Standards and Certifications

	Safety
	EN 62368-1(LVD)

	EMI
	FCC Part 15 Subpart B Class A EN 55032 Class A

	EMS
	IEC(EN)61000-4-2(ESD): ±8kV Contact, ±8kV Indirect,±15kV Air
IEC(EN)61000-4-3(RS):10V/m(80～1000MHz)
IEC(EN)61000-4-4(EFT): power line:±4kV; data line:±2kV
IEC(EN)61000-4-5(Surge): power:±6kV CM/±4kV DM; data:±4kV
IEC(EN)61000-4-6(RF conduction):3V(10kHz～150kHz),10V(150kHz～80MHz)
IEC(EN)61000-4-16(Common mode conduction):30V cont. 300V,1s
IEC(EN )61000-4-8

	Shock
	IEC 60068-2-27

	Freefall
	IEC 60068-2-32

	Vibration
	IEC 60068-2-6

	MTBF

	Time
	300 000hrs

	Warranty

	Warranty Period
	5years


SOFTWARE:
	Port Features 
	IEEE 802.3x Flow control

	
	Interface counters

	
	Storm Control

	Link Aggregation 
	Static Aggregation

	
	Dynamic Aggregation, LACP

	
	Supports up to 4 aggregation groups, each group up to 8 ports
Load balancing

	MAC Address Table
	Static MAC Address
MAC Binding

	Mirroring 
	Port-based
One-to-one Mirroring, Many-to-one Mirroring

	Spanning Tree 
	IEEE802.1d STP

	
	IEEE802.1w RSTP

	
	IEEE802.1s MSTP

	ERPS (G.8032) 
	Single Ring, Sub-Ring, Multi-Ring

	
	Recovery Time < 50ms

	LLDP 
	LLDP

	
	LLDP-MED

	Loop Protection 
	Supported

	VLAN 
	4094 VLAN

	
	Port-based VLAN

	
	GVRP

	IGMP 
	Snooping IGMP V1 Snooping

	
	IGMP V2 Snooping

	
	IGMP V3 Snooping

	
	Source Port Check

	
	IGMP Fast Leave

	Security
	

	ACL 
	ACL (IP Standard ACL), IPv4/IPv6

	
	MAC extend ACL

	
	IP extend ACL

	
	L2, L3, L4 fields match

	QoS 
	QoS Class, Remarking

	
	SP, WRR queue scheduling

	
	Ingress port-based rate-limit

	
	Ingress priority-based rate-limit

	
	Egress port-based rate-limit

	
	Egress queue-based rate-limit

	
	Policy-based QoS

	
	Storm Control

	
	8 queues per port

	802.1X
	Port-based

	User management 
	Password protection

	SNMP 
	SNMP V1/V2c/V3

	RMON 
	Statistics Group

	
	History Group

	
	Alarm Group

	
	Events Group

	Web management 
	HTTP V1.1, HTTPS

	Firmware Upgrade 
	Reversion Upgrade

	CLI 
	Support

	Syslog/Debug 
	Support

	Diagnosis 
	Ping (IPv4), ping (IPv6)

	
	Trace route(IPv4)

	Management
	

	NTP 
	SNTP 

	Telnet 
	Telnet Server

	TFTP 
	TFTP Client

	SSH 
	SSH Server


Dimensions
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Order Information
	Specification
	Model No.

	L2 Managed Industrial Switch
8 Port 10/100/1000Base TX+2 Port 100/1000 SFP
	EL82MGI V3
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