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EL242GSPMI an hardened 26-Port Industrial Ethernet Switch, provides non-blocking wire-speed performance in harsh industrial environment. It also provides 24-Port 10/100/1000BASE-TX RJ45(PoE) +2G SFP delivered in an IP40 rugged, strong case with redundant power system. It’s suitable for such applications as surveillance system deployments, control management and wireless service in climatically demanding environments with wide temperature range from -40℃ to 75℃Interface
· 24-port 10/100/1000Base-Tx RJ-45 with auto negotiation and auto-MDI/ MDI-X function
· 2G SFP uplink (automatically 100Mbps/1000Mbps SFP module)
· 1-24 Port PoE output,each max.30W
· PoE budget: 380W max.
Industrial conformance
· AC110-240V redundant power input
· - 40℃ to 75℃ operating temperature
· IP40 aluminum housing 
· Supports ESD protection: contact 8KV, air 12KV
· Supports Surge protection: CM±4KV, DM±2KV
· Free Fall, Shock and Vibration Stability
· 19“ Rak-mountable hardware design


The EL242GSPMI provides the flexibility to all kinds of 10/100/1000Mbps Ethernet Media on SFP port and performs highly stable fiber performance
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YOUR ONE-STOP ICT CONNECTIVITY SOLUTION PROVIDER

The EL242GSPMI is packaged in a compact IP40 case that allows bracket mounting to cabinet. It provides power supply AC100-240V input
SPECIFICATIONS:
	Model No.
	EL242GSPMI

	1000Base-TX Port
	24 Port 10/100/1000 RJ45

	1000Base-FX Port
	2G SFP 100/1000

	PoE Specification
	PoE ports:1-24 port support PoE
Max. 15.4 watts (IEEE 802.3af)
Max. 30 watts (IEEE 802.3at)
Power Pin Assignment:1/2+;3/6-
PoE budget: Max.380W

	
Performance Specification
	Bandwidth: 56Gbps 
Packet Buffer Memory: 12Mbit
Packet Forwarding Rate: 42Mpps
MAC Address Table: 8K

	Installation
	Rak mounted

	Maximum Frame Size
	10240bytes packet size

	Flow Control
	Back pressure for half duplex, IEEE 802.3x pause frame for full duplex

	Enclosure
	IP40 Aluminum housing

	
LED Indicator
	Power: Red
Fiber: Link (Green)
Ethernet: Yellow 

	Power Input
	AC110-240V
Supports built-in over-current 4.0A protection
Supports reverse connection protection

	Power Consumption
	< 400W

	Surge protection
	 ± 4KV

	
Network Protocols
	IEEE802.3 10BASE-T; 
IEEE802.3i 10Base-T; 
IEEE802.3u;100Base-TX/FX; 
IEEE802.3ab 1000Base-T;  
IEEE802.3z 1000Base-X; 
IEEE802.3x;

	Network cables
	10BASE-T: Cat3,4,5 UTP(≤100 meter)     
100BASE-TX: Cat5 or later UTP(≤100meter)
1000BASE-TX: Cat6 or later UTP(≤100 meter)

	

Industry Standard
	FCC CFR47 Part 15,EN55032 Class A 
IEC61000-4-2 (ESD): ±8kV (contact), ±12kV (air)
IEC61000-4-3 (RS): 10V/m (80~1000MHz)
IEC61000-4-4 (EFT): Power Port: ±4kV; Data Port: ±2kV
IEC61000-4-5 (Surge): Power Port: ±2kV/DM, ±4kV/CM; Data Port: ±2kV
IEC61000-4-6 (CS): 3V (10kHz-150kHz); 10V (150kHz-80MHz)
IEC61000-4-16 (Common mode conduction): 30V (cont.), 300V (1s)

	MTBF
	300,000hours

	Dimensions (W x D x H)
	442×325×44mm

	Weight
	Product Weight: 4.5KG
Packing Weight: 5.0KG

	Working Environment

	Working temperature: -40～75℃ ;  
Storage temperature: -40～75℃
Relative Humidity: 5%~95 %( no condensation)


SOFTWARE:
	[bookmark: OLE_LINK1]Port Features 
	IEEE 802.3x Flow control

	
	Interface counters

	
	Storm Control

	Link Aggregation 
	Static Aggregation

	
	Dynamic Aggregation, LACP

	
	Supports up to 4 aggregation groups, each group up to 8 ports
Load balancing

	MAC Address Table
	Static MAC Address
MAC Binding

	Mirroring 
	Port-based
One-to-one Mirroring, Many-to-one Mirroring

	Spanning Tree 
	IEEE802.1d STP

	
	IEEE802.1w RSTP

	
	IEEE802.1s MSTP

	ERPS (G.8032) 
	Single Ring, Sub-Ring, Multi-Ring

	
	Recovery Time < 50ms

	LLDP 
	LLDP

	
	LLDP-MED

	Loop Protection 
	Supported

	VLAN 
	4094 VLAN

	
	Port-based VLAN

	
	GVRP

	Protocol VLAN 
	MAC-based VLAN

	
	IP Subnet-based VLAN

	
	Voice VLAN

	Port Isolate 
	Support

	IGMP 
	Snooping IGMP V1 Snooping

	
	IGMP V2 Snooping

	
	IGMP V3 Snooping

	
	Source Port Check

	
	IGMP Fast Leave

	
	IGMP Filter

	MLD Snooping 
	MLD V1 Snooping

	
	MLD V2 Snooping

	
	Source Port Check

	
	MLD Fast Leave

	
	MLD Filter

	Security
	

	ACL 
	ACL (IP Standard ACL), IPv4/IPv6

	
	MAC extend ACL

	
	IP extend ACL

	
	L2, L3, L4 fields match

	
	log, redirection, mirroring, speed limit

	QoS 
	QoS Class, Remarking

	
	SP, WRR queue scheduling

	
	Ingress port-based rate-limit

	
	Ingress priority-based rate-limit

	
	Egress port-based rate-limit

	
	Egress queue-based rate-limit

	
	Policy-based QoS

	
	Storm Control

	
	8 queues per port

	802.1X
	Port-based

	User management 
	Password protection

	SNMP 
	SNMP V1/V2c/V3

	RMON 
	Statistics Group

	
	History Group

	
	Alarm Group

	
	Events Group

	Web management 
	HTTP V1.1, HTTPS

	Firmware Upgrade 
	Reversion Upgrade

	IPv4/IPv6 
	Support

	CLI 
	Support

	Syslog/Debug 
	Support

	Diagnosis 
	Ping (IPv4), ping (IPv6)

	
	Trace route(IPv4)

	Management
	

	NTP 
	NTP Client

	DHCP 
	DHCPv4 Client, DHCPv6 Client

	DHCP Snooping 
	DHCP snooping table

	
	Trust Port

	Telnet 
	Telnet Server

	TFTP 
	TFTP Client

	SSH 
	SSH Server


Dimensions
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Ordering Information
	EL242GSPMI
	24-Port 10/100/100BASE-TX+2G SFP Managed Industrial PoE Switch
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