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EL1042F-SFP                                4-Port RJ45+2 SFP Fast Industrial Switch
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YOUR ONE-STOP ICT CONNECTIVITY SOLUTION PROVIDER

EL1042F-SFP is an integrated industrial switch (Industrial media converter) with 4 Port RJ45 100Mbps+2 Port SFP uplink. This product is mainly developed for the application of point-to-point networks, star networks, tree networks and chain networks in the industrial field. The longest optical communication distance can reach 120KM. Its high-performance switching engine has an IP40 protection-grade casing, a fanless design and an efficient corrugated aluminum alloy casing heat dissipation surface. The power input end has over-current, over-voltage and EMC protection, and the RJ45 port has excellent EMC protection performance, making this series of products able to adapt to harsh and dangerous industrial environments. Provide reliable and convenient solutions for users' Ethernet device networking. 
Interface
· 4*10/100BaseT(X),Automatic detection, Full/half duplex MDI/MDI-x adaptive
· 2*100Base-FX Port , SFP 
Industrial conformance
· 9V to 52V DC, redundant power input
· -40℃ to 75℃ operating temperature
· IP40 aluminum housing 
· Supports 6KV DC Ethernet ESD protection
· Supports 6KV DC EFT protection for power line
· Free Fall, Shock and Vibration Stability
· DIN-rail hardware design

SPECIFICATIONS:
	Product Name
	4 Port RJ45+2 Port SFP Industrial Switch

	Model No.
	EL1042F-SFP

	Ethernet interface

	RJ45 Port
	4*10/100BaseT(X),Automatic detection, Full/half duplex MDI/MDI-x adaptive

	Optical port
	2*100Base-FX SFP

	Power Parameters
	

	Power
	Connection: 1x removable 5-contact terminal block(s)
Input voltage: DC9 to 52V redundant power support reverse connection protection

	LED Indicator
	Power: Green
Link: Green 

	Standards

	Network Protocols
	IEEE802.3 10BASE-T;100BASE-T IEEE802.3i 10Base-T;IEEE802.3u;
IEEE802.3x; 

	Twisted Pair
	10BASE-T: Cat3,4,5 UTP(≤100 meter)
100BASE-TX: Cat5 or later UTP(≤100 meter)

	Switch Properties

	Processing Type:
	Store and Forward

	MAC Table Size
	2K 

	Packet Buffer Size
	2Mbit

	Bandwidth
	1.6G

	Switching Delay
	＜10μs

	Power Consume
	＜5W

	Physical Characteristics

	Protection level
	IP40 

	Enclosure
	Wavy aluminum alloy

	Installation
	Push-in DIN rail

	Weigh
	0.4kg

	Dimensions
	115x70x30mm（length x width x height)

	Environmental Limits

	Working temperature
	-40～75℃ （-40～167 °F）

	Storage Temperature (package included)
	-40 to 85°C (-40 to 185°F)

	Ambient Relative Humidity
	5 to 95% (non-condensing)

	Standards and Certifications

	Safety
	EN 62368-1(LVD)

	EMI
	FCC Part 15 Subpart B Class A, EN 55032 Class A

	EMS
	IEC(EN)61000-4-2(ESD): ±8kV Contact, ±8kV Indirect,±15kV Air
IEC(EN)61000-4-3(RS):10V/m(80～1000MHz)
IEC(EN)61000-4-4(EFT): power line:±4kV; data line:±2kV
IEC(EN)61000-4-5(Surge): power:±6kV CM/±4kV DM; data:±4kV
IEC(EN)61000-4-6(RF conduction):3V(10kHz～150kHz),10V(150kHz～80MHz)
IEC(EN)61000-4-16(Common mode conduction):30V cont. 300V,1s
IEC(EN )61000-4-8

	Shock
	IEC 60068-2-27

	Freefall
	IEC 60068-2-32

	Vibration
	IEC 60068-2-6

	MTBF

	Time
	300 000hrs

	Warranty

	Warranty Period
	5years
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Booking Information:
	Model No.
	Specification

	EL1042F-SFP
	4 Port 10/100 Base -T +2-Port optical SFP Fast Industrial Switch

	EL1042F-SC2
	4 Port 10/100 Base -T +2-Port optical 1*9 (Multi Mode, (Tx/Rx1310nm), Dual fiber, SC2) Fast Industrial Switch, ST/FC Interface is optional

	EL1042F-SC20
	4 Port 10/100 Base -T +2-Port optical 1*9 (Single Mode, (Tx/Rx1310nm), Dual fiber, SC20) Fast Industrial Switch, ST/FC Interface is optional

	EL1042F-SC20A
	4 Port 10/100 Base -T +2-Port optical 1*9 (Single Mode, (Rx1310nm/A), Single fiber, SC20) Fast Industrial Switch, ST/FC Interface is optional

	EL1042F-SC20B
	4 Port 10/100 Base -T +2-Port optical 1*9 (Single Mode, (Tx1550nm/B), Single fiber, SC20) Fast Industrial Switch, ST/FC Interface is optional
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